(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Si7223DN"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 22.86 5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Si7223DN"
				(at 22.86 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Si7223DN"
				(at 22.86 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/2606257.pdf"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual MOSFET, P Channel, 30 V, 30 V, 6 A, 6 A, 0.022 ohm"
				(at 22.86 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI7223DN-T1-GE3"
				(at 22.86 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Vishay"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SEMICONDUCTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Si7223DN_1_1"
				(pin passive line
					(at 13.97 -1.27 180)
					(length 2.54)
					(name "S1")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "G1")
					(number "2")
				)
				(pin passive line
					(at 13.97 -10.16 180)
					(length 2.54)
					(name "S2")
					(number "3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "G2")
					(number "4")
				)
				(pin passive line
					(at 13.97 -5.08 180)
					(length 2.54)
					(name "D2")
					(number "5")
				)
				(pin passive line
					(at 13.97 3.81 180)
					(length 2.54)
					(name "D1")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
