(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SIS862DN-T1-GE3"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Q"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SIS862DN-T1-GE3"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SIS862DN-T1-GE3"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/63346/sis862dn.pdf"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power MOSFET, N Channel, 60 V, 40 A, 0.007 ohm, PowerPAK 1212, Surface Mount"
				(at 15.24 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SIS862DN-T1-GE3"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Vishay"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSISTOR, SEMICONDUCTOR, MOSFET, PMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SIS862DN-T1-GE3_1_1"
				(pin passive line
					(at 6.35 -2.54 90)
					(length 2.54)
					(name "S")
					(number "1")
				)
				(pin passive line
					(at 6.35 -2.54 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 6.35 -2.54 90)
					(length 2.54)
					(hide yes)
					(name "S")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "4")
				)
				(pin passive line
					(at 6.35 7.62 270)
					(length 2.54)
					(name "D")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
