(footprint "diodes_dmp6023le" (version 20221018) (generator opencad-lib)
  (layer "F.Cu")
  (descr "DMP6023LE-13 60V P-channel MOSFET (SOT-223). SOT-223: lead pads 1.2x1.6 at pitch 2.3, tab pad 3.3x1.6, row centres 6.4 apart (manufacturer suggested pad layout).")
  (tags "DMP6023LE-13 MOSFET P-channel SOT-223")
  (attr smd)
  (fp_text reference "REF**" (at 0 -5.0) (layer "F.SilkS"))
  (fp_text value "diodes_dmp6023le" (at 0 5.0) (layer "F.Fab"))
  (pad "1" smd rect (at -2.3 3.2) (size 1.2 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0 3.2) (size 1.2 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 2.3 3.2) (size 1.2 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0 -3.2) (size 3.3 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
)
