(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PTC_3A_1210"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "F"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PTC_3A_1210"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PTC_3A_1210"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=4b6f5b2d-4096-4267-a055-9f2e3cb58660&filename=littelfuse-ptc-1210l-datasheet"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Resettable Fuse, PPTC, 1210 (3225 Metric), PolySwitch 1210L Series, 16 VDC, 1.5 A, 3 A, 0.3 s"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1210L150/16WR"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Littelfuse"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "FUSE, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PTC_3A_1210_0_1")
			(symbol "PTC_3A_1210_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.27)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
