(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "F_10A_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "F"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "F_10A_1206"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "F_10A_1206"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://us.schurter.com/pdf/english/typ_UST_1206.pdf"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fuse, Surface Mount, 10 A, Slow Blow, 32 VAC, 63 VDC, 1206 (3216 Metric), UST 1206"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Schurter"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "3413.0328.22"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "FUSE, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "F_10A_1206_0_1")
			(symbol "F_10A_1206_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.27)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
