(footprint "FUSC_BOURNS_SF-0603S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0603 (1608mm), Body 1.6 x 0.8mm, Slow Blow Thin Film Chip Fuse, SinglFuse SF-0603S Series")
	(property "Reference" "REF**"
		(at 0 -1.425 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSC_BOURNS_SF-0603S"
		(at 0 1.425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.725 0)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.725 0)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
