(footprint "FUSH_LITTELFUSE_01110501"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Horizontal Fuse Holder For 6.4x8.8mm Subminiature Fuses")
	(property "Reference" "REF**"
		(at 0.45 -4.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_LITTELFUSE_01110501"
		(at 0.45 4.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at 0 -2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at 0 2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.2 2.7) (xy 3.1 2.7) (xy 3.1 -2.7) (xy -2.2 -2.7)
			)
		)
	)
	(embedded_fonts no)
)
