(footprint "FUSH_LITTELFUSE_109001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Rivet/Eyelet Mount Fuse Clips for 20.6mm (0.81\" or 13/16\") Diameter Fuses")
	(property "Reference" "REF**"
		(at -0.300005 -12.37501 0)
		(layer "F.SilkS")
	)
	(property "Value" "FUSH_LITTELFUSE_109001"
		(at -0.300005 12.37501 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole roundrect
		(at 1.655 0)
		(size 19.05 22.35)
		(drill 6.8
			(offset -1.655 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
)
