(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74HC00_DHVQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74HC00_DHVQFN"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74HC00_DHVQFN"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mouser.com/datasheet/2/916/74HC_HCT00-1318972.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Logic gate"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74HC00BQ,115"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74HC00_DHVQFN_1_1"
				(text "4xNAND"
					(at 3.81 -13.97 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1A")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "1B")
					(number "2")
				)
				(pin passive line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "~{1Y}")
					(number "3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "2A")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "2B")
					(number "5")
				)
				(pin passive line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "~{2Y}")
					(number "6")
				)
				(pin passive line
					(at 15.24 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin passive line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "~{3Y}")
					(number "8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "3A")
					(number "9")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "3B")
					(number "10")
				)
				(pin passive line
					(at 15.24 -20.32 180)
					(length 2.54)
					(name "~{4Y}")
					(number "11")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "4A")
					(number "12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "4B")
					(number "13")
				)
				(pin passive line
					(at 15.24 0 180)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
				(pin passive line
					(at 15.24 -25.4 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
