(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LCX07_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LCX07_QFN"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LCX07_QFN"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/74LCX07_D-2309542.pdf"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buffer, Non-Inverting 6 Element 1 Bit per Element Open Drain Output 14-DQFN (3x2.5)"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LCX07BQX"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LCX07_QFN_1_0"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "2")
				)
			)
			(symbol "74LCX07_QFN_1_1")
			(symbol "74LCX07_QFN_2_0"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "4")
				)
			)
			(symbol "74LCX07_QFN_2_1")
			(symbol "74LCX07_QFN_3_0"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(symbol "74LCX07_QFN_3_1")
			(symbol "74LCX07_QFN_4_0"
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "9")
				)
			)
			(symbol "74LCX07_QFN_4_1")
			(symbol "74LCX07_QFN_5_0"
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "11")
				)
			)
			(symbol "74LCX07_QFN_5_1")
			(symbol "74LCX07_QFN_6_0"
				(pin open_collector line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "13")
				)
			)
			(symbol "74LCX07_QFN_6_1")
			(symbol "74LCX07_QFN_7_0"
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
				(pin no_connect line
					(at 2.54 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "DAP")
					(number "15")
				)
			)
			(symbol "74LCX07_QFN_7_1")
			(embedded_fonts no)
		)
)
