(footprint "Spacer_Drill3.7mm_H7mm_9774070151"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Spacer M=3 h=7mm fi=5.1mm")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Spacer_Drill3.7mm_H7mm_9774070151"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -9.6 6.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.6 7.7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.6 8.9 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.7 -1.7)
		(size 0.62 0.62)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.250195 1.279127)
				(mid 0.285453 0.294389)
				(end 1.266786 -0.24747)
				(width 0.2)
			)
			(gr_arc
				(start -0.34334 1.279127)
				(mid 0.218448 0.232561)
				(end 1.259603 -0.339191)
				(width 0.2)
			)
			(gr_arc
				(start -0.436309 1.279127)
				(mid 0.152481 0.169693)
				(end 1.255279 -0.431435)
				(width 0.2)
			)
			(gr_arc
				(start -0.529126 1.279127)
				(mid 0.087542 0.105784)
				(end 1.253811 -0.524161)
				(width 0.2)
			)
			(gr_arc
				(start -0.621807 1.279127)
				(mid 0.0309 0.033527)
				(end 1.275473 -0.621136)
				(width 0.2)
			)
			(gr_arc
				(start -0.71437 1.279127)
				(mid -0.037758 -0.026651)
				(end 1.263664 -0.711602)
				(width 0.2)
			)
			(gr_arc
				(start -0.806826 1.279127)
				(mid -0.105837 -0.087395)
				(end 1.253435 -0.802342)
				(width 0.2)
			)
			(gr_arc
				(start -0.899187 1.279127)
				(mid -0.165236 -0.156885)
				(end 1.267475 -0.897258)
				(width 0.2)
			)
			(gr_arc
				(start -0.991463 1.279127)
				(mid -0.228522 -0.222449)
				(end 1.270645 -0.990112)
				(width 0.2)
			)
			(gr_arc
				(start -1.083663 1.279127)
				(mid -0.294507 -0.285313)
				(end 1.266278 -1.081674)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 -0.250195)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 1.279127)
				(end -1.083663 1.279127)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -1.7 1.7 90)
		(size 0.62 0.62)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.250195 1.279127)
				(mid 0.285453 0.294389)
				(end 1.266786 -0.24747)
				(width 0.2)
			)
			(gr_arc
				(start -0.34334 1.279127)
				(mid 0.218448 0.232561)
				(end 1.259603 -0.339191)
				(width 0.2)
			)
			(gr_arc
				(start -0.436309 1.279127)
				(mid 0.152481 0.169693)
				(end 1.255279 -0.431435)
				(width 0.2)
			)
			(gr_arc
				(start -0.529126 1.279127)
				(mid 0.087542 0.105784)
				(end 1.253811 -0.524161)
				(width 0.2)
			)
			(gr_arc
				(start -0.621807 1.279127)
				(mid 0.0309 0.033527)
				(end 1.275473 -0.621136)
				(width 0.2)
			)
			(gr_arc
				(start -0.71437 1.279127)
				(mid -0.037758 -0.026651)
				(end 1.263664 -0.711602)
				(width 0.2)
			)
			(gr_arc
				(start -0.806826 1.279127)
				(mid -0.105837 -0.087395)
				(end 1.253435 -0.802342)
				(width 0.2)
			)
			(gr_arc
				(start -0.899187 1.279127)
				(mid -0.165236 -0.156885)
				(end 1.267475 -0.897258)
				(width 0.2)
			)
			(gr_arc
				(start -0.991463 1.279127)
				(mid -0.228522 -0.222449)
				(end 1.270645 -0.990112)
				(width 0.2)
			)
			(gr_arc
				(start -1.083663 1.279127)
				(mid -0.294507 -0.285313)
				(end 1.266278 -1.081674)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 -0.250195)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 1.279127)
				(end -1.083663 1.279127)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.7 -1.7 270)
		(size 0.62 0.62)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.250195 1.279127)
				(mid 0.285453 0.294389)
				(end 1.266786 -0.24747)
				(width 0.2)
			)
			(gr_arc
				(start -0.34334 1.279127)
				(mid 0.218448 0.232561)
				(end 1.259603 -0.339191)
				(width 0.2)
			)
			(gr_arc
				(start -0.436309 1.279127)
				(mid 0.152481 0.169693)
				(end 1.255279 -0.431435)
				(width 0.2)
			)
			(gr_arc
				(start -0.529126 1.279127)
				(mid 0.087542 0.105784)
				(end 1.253811 -0.524161)
				(width 0.2)
			)
			(gr_arc
				(start -0.621807 1.279127)
				(mid 0.0309 0.033527)
				(end 1.275473 -0.621136)
				(width 0.2)
			)
			(gr_arc
				(start -0.71437 1.279127)
				(mid -0.037758 -0.026651)
				(end 1.263664 -0.711602)
				(width 0.2)
			)
			(gr_arc
				(start -0.806826 1.279127)
				(mid -0.105837 -0.087395)
				(end 1.253435 -0.802342)
				(width 0.2)
			)
			(gr_arc
				(start -0.899187 1.279127)
				(mid -0.165236 -0.156885)
				(end 1.267475 -0.897258)
				(width 0.2)
			)
			(gr_arc
				(start -0.991463 1.279127)
				(mid -0.228522 -0.222449)
				(end 1.270645 -0.990112)
				(width 0.2)
			)
			(gr_arc
				(start -1.083663 1.279127)
				(mid -0.294507 -0.285313)
				(end 1.266278 -1.081674)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 -0.250195)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 1.279127)
				(end -1.083663 1.279127)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.7 1.7 180)
		(size 0.62 0.62)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.250195 1.279127)
				(mid 0.285453 0.294389)
				(end 1.266786 -0.24747)
				(width 0.2)
			)
			(gr_arc
				(start -0.34334 1.279127)
				(mid 0.218448 0.232561)
				(end 1.259603 -0.339191)
				(width 0.2)
			)
			(gr_arc
				(start -0.436309 1.279127)
				(mid 0.152481 0.169693)
				(end 1.255279 -0.431435)
				(width 0.2)
			)
			(gr_arc
				(start -0.529126 1.279127)
				(mid 0.087542 0.105784)
				(end 1.253811 -0.524161)
				(width 0.2)
			)
			(gr_arc
				(start -0.621807 1.279127)
				(mid 0.0309 0.033527)
				(end 1.275473 -0.621136)
				(width 0.2)
			)
			(gr_arc
				(start -0.71437 1.279127)
				(mid -0.037758 -0.026651)
				(end 1.263664 -0.711602)
				(width 0.2)
			)
			(gr_arc
				(start -0.806826 1.279127)
				(mid -0.105837 -0.087395)
				(end 1.253435 -0.802342)
				(width 0.2)
			)
			(gr_arc
				(start -0.899187 1.279127)
				(mid -0.165236 -0.156885)
				(end 1.267475 -0.897258)
				(width 0.2)
			)
			(gr_arc
				(start -0.991463 1.279127)
				(mid -0.228522 -0.222449)
				(end 1.270645 -0.990112)
				(width 0.2)
			)
			(gr_arc
				(start -1.083663 1.279127)
				(mid -0.294507 -0.285313)
				(end 1.266278 -1.081674)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 -0.250195)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 1.279127)
				(end -1.083663 1.279127)
				(width 0.2)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6 6)
		(drill 3.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_9774070151.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
