(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM4050-N-Q1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 11.43 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM4050-N-Q1"
				(at 11.43 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM4050-N-Q1"
				(at 11.43 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm4050-n-q1.pdf"
				(at 11.43 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive, 50-ppm/°C precision micropower 5V shunt voltage reference"
				(at 11.43 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM4050QAEM3-5.0/NOPB "
				(at 11.43 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 11.43 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 11.43 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 11.43 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM4050-N-Q1_1_1"
				(text "C"
					(at 1.27 -1.27 0)
				)
				(text "A"
					(at 1.27 -6.35 0)
				)
				(pin passive line
					(at 0 0 270)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -7.62 90)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -7.62 90)
					(length 2.54)
					(hide yes)
					(name "")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
)
