(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP6541_SOT23-5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP6541_SOT23-5"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP6541_SOT23-5"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1641674.pdf"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Push-Pull Output Comparator, 1,6V to 5.5V, SOT-23-5"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP6541T-E/OT"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT,  IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP6541_SOT23-5_1_1"
				(text "+"
					(at 2.54 -1.016 0)
				)
				(text "-"
					(at 2.54 -3.302 0)
				)
				(pin output line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "4")
				)
			)
			(symbol "MCP6541_SOT23-5_2_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VSS")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
