(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PD0922J5050S2HF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PD0922J5050S2HF"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PD0922J5050S2HF"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/21/PD0922J5050S2HF_97_D-3011607.pdf"
				(at 30.48 -10.795 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Power Divider 950 MHz ~ 2.15 GHz Isolation (Min) 9dB, 12dB Return Loss 0805 (2012 Metric)"
				(at 40.005 -18.415 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -13.335 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -15.875 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PD0922J5050S2HF"
				(at 40.005 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Anaren"
				(at 33.655 -5.715 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PD0922J5050S2HF_1_1"
				(text "-3 dB"
					(at 7.62 -3.175 0)
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 15.24 0 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
