(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "THVD1450_VSON"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "THVD1450_VSON"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "THVD1450_VSON"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1450.pdf?ts=1705935202714&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTHVD1450%253Futm_source%253Dgoogle%2526utm_medium%253Dcpc%2526utm_campaign%253Dasc-null-null-gpn_en-cpc-pf-google-wwe%2526utm_content%253Dthvd1450%2526ds_k%253DTHVD1450%2526dcm%253Dyes%2526gad_source%253D1%2526gclid%253DCj0KCQiAwbitBhDIARIsABfFYIJ1r-KNvaFopPvdPXOqr1zQUjL1eW4ZJ8pxsixczrV4z0lGKUA5MqYaAgV2EALw_wcB%2526gclsrc%253Daw.ds"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "3.3-V to 5-V RS-422/RS-485 Interface Transceivers with Auto-direction Control"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "THVD1450DRBR"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, DRIVER, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "THVD1450_VSON_1_1"
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(name "R")
					(number "1")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "~{RE}")
					(number "2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DE")
					(number "3")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D")
					(number "4")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "A")
					(number "6")
				)
				(pin passive line
					(at 15.24 -6.35 180)
					(length 2.54)
					(name "B")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
