(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "LM5164"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "IC"
  			(at 11.43 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 11.43 -24.13 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "SIMPLE SWITCHER® 4.2-V to 65-V, 2-A Synchronous Step-down Converter"
  			(at 0 0 0)
  		)
  		(symbol "LM5164_1_0"
  			(pin input line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "VIN")
  				(number "2")
  			)
  			(pin input line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "EN/UVLO")
  				(number "3")
  			)
  			(pin input line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "RON")
  				(number "4")
  			)
  			(pin output line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "PGOOD")
  				(number "6")
  			)
  			(pin output line
  				(at 27.94 -2.54 180)
  				(length 5.08)
  				(name "SW")
  				(number "8")
  			)
  			(pin input line
  				(at 27.94 -7.62 180)
  				(length 5.08)
  				(name "BST")
  				(number "7")
  			)
  			(pin input line
  				(at 27.94 -12.7 180)
  				(length 5.08)
  				(name "FB")
  				(number "5")
  			)
  			(pin power_in line
  				(at 27.94 -17.78 180)
  				(length 5.08)
  				(name "GND")
  				(number "1")
  			)
  			(pin power_in line
  				(at 27.94 -20.32 180)
  				(length 5.08)
  				(name "EP")
  				(number "9")
  			)
  		)
  		(embedded_fonts no)
  	)
)
