(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "TPS259573"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "IC"
  			(at 10.16 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 10.16 -24.13 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "2.7V to 18V, 4A, 34-mOhm eFuse With Fast Programmable Overvoltage Protection"
  			(at 0 0 0)
  		)
  		(symbol "TPS259573_1_0"
  			(pin input line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "IN")
  				(number "3")
  			)
  			(pin input line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "IN")
  				(number "4")
  			)
  			(pin input line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "~{EN}/OVLO")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "dVdT")
  				(number "1")
  			)
  			(pin output line
  				(at 25.4 -2.54 180)
  				(length 5.08)
  				(name "OUT")
  				(number "5")
  			)
  			(pin output line
  				(at 25.4 -7.62 180)
  				(length 5.08)
  				(name "~{FLT}")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at 25.4 -12.7 180)
  				(length 5.08)
  				(name "ILM")
  				(number "7")
  			)
  			(pin power_in line
  				(at 25.4 -17.78 180)
  				(length 5.08)
  				(name "GND")
  				(number "8")
  			)
  			(pin power_in line
  				(at 25.4 -20.32 180)
  				(length 5.08)
  				(name "GND")
  				(number "9")
  			)
  		)
  		(embedded_fonts no)
  	)
)
