(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "TPS26600PWP"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "IC"
  			(at 10.16 1.27 0)
  		)
  		(property "Value" "${DEVICE}"
  			(at 10.16 -36.83 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "60V, 2A Industrial eFuse With Integrated Reverse Input Polarity Protection"
  			(at 0 0 0)
  		)
  		(symbol "TPS26600PWP_1_0"
  			(pin input line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "IN")
  				(number "1")
  			)
  			(pin input line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "IN")
  				(number "2")
  			)
  			(pin input line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "UVLO")
  				(number "3")
  			)
  			(pin input line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "OVP")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "dVdT")
  				(number "12")
  			)
  			(pin input line
  				(at -5.08 -25.4 0)
  				(length 5.08)
  				(name "MODE")
  				(number "6")
  			)
  			(pin passive line
  				(at -5.08 -30.48 0)
  				(length 5.08)
  				(name "RTN")
  				(number "8")
  			)
  			(pin power_in line
  				(at -5.08 -33.02 0)
  				(length 5.08)
  				(name "PwPd")
  				(number "17")
  			)
  			(pin output line
  				(at 25.4 -2.54 180)
  				(length 5.08)
  				(name "OUT")
  				(number "15")
  			)
  			(pin output line
  				(at 25.4 -5.08 180)
  				(length 5.08)
  				(name "OUT")
  				(number "16")
  			)
  			(pin output line
  				(at 25.4 -10.16 180)
  				(length 5.08)
  				(name "~{FLT}")
  				(number "14")
  			)
  			(pin input line
  				(at 25.4 -15.24 180)
  				(length 5.08)
  				(name "~{SHDN}")
  				(number "7")
  			)
  			(pin output line
  				(at 25.4 -20.32 180)
  				(length 5.08)
  				(name "IMON")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at 25.4 -25.4 180)
  				(length 5.08)
  				(name "ILIM")
  				(number "11")
  			)
  			(pin passive line
  				(at 25.4 -27.94 180)
  				(length 5.08)
  				(name "N.C.")
  				(number "4")
  			)
  			(pin passive line
  				(at 25.4 -30.48 180)
  				(length 5.08)
  				(name "N.C.")
  				(number "13")
  			)
  			(pin power_in line
  				(at 25.4 -33.02 180)
  				(length 5.08)
  				(name "GND")
  				(number "9")
  			)
  		)
  		(embedded_fonts no)
  	)
)
