(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RF_COM-13909"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RF_COM-13909"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RF_COM-13909"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Wireless/General/RFM69HCW-V1.1.pdf"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "COM-13909"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "SparkFun"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RF_COM-13909_1_1"
				(pin power_in line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "MISO")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "MOSI")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCK")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "NSS")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RESET")
					(number "6")
				)
				(pin bidirectional line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "DIO5")
					(number "7")
				)
				(pin passive line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "ANT")
					(number "9")
				)
				(pin passive line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "DIO3")
					(number "11")
				)
				(pin bidirectional line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "DIO4")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "3.3V")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DIO0")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DIO1")
					(number "15")
				)
				(pin bidirectional line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "DIO2")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
