(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_Bluetooth_ESP32-WROOM-32"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_Bluetooth_ESP32-WROOM-32"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_Bluetooth_ESP32-WROOM-32"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver module"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ESP32-WROOM-32"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Espressif Systems"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MODULE, BLUETOOTH, RF, ANTENNA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_Bluetooth_ESP32-WROOM-32_1_1"
				(pin power_in line
					(at 22.86 -43.18 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "3V3")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin input line
					(at 22.86 0 180)
					(length 2.54)
					(name "SENSOR_VP")
					(number "4")
				)
				(pin input line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "SENSOR_VN")
					(number "5")
				)
				(pin bidirectional line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "IO34")
					(number "6")
				)
				(pin bidirectional line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "IO35")
					(number "7")
				)
				(pin bidirectional line
					(at 22.86 -33.02 180)
					(length 2.54)
					(name "IO32")
					(number "8")
				)
				(pin bidirectional line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "IO33")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "IO25")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 -38.1 180)
					(length 2.54)
					(name "IO26")
					(number "11")
				)
				(pin bidirectional line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "IO27")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IO14")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IO12")
					(number "14")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IO13")
					(number "16")
				)
				(pin bidirectional line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "SHD/SD2")
					(number "17")
				)
				(pin bidirectional line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "SWP/SD3")
					(number "18")
				)
				(pin bidirectional line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "SCS/CMD")
					(number "19")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "SCK/CLK")
					(number "20")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "SDO/SD0")
					(number "21")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "SDI/SD1")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IO15")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IO2")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IO0")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "IO4")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IO16")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "IO17")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "IO5")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "IO18")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "IO19")
					(number "31")
				)
				(pin no_connect line
					(at 20.32 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "IO21")
					(number "33")
				)
				(pin bidirectional line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "RXD0")
					(number "34")
				)
				(pin bidirectional line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "TXD0")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "IO22")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "IO23")
					(number "37")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
			)
			(embedded_fonts no)
		)
)
