(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_24MHz_TXC_7C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 26.035 -1.905 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_24MHz_TXC_7C"
				(at 26.035 -12.065 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_24MHz_TXC_7C"
				(at 26.035 -14.605 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.txccorp.com/download/products/oscillators/2015TXC_7C_57.pdf"
				(at 26.035 -17.145 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Oscillator, 24 MHz, 50 ppm, SMT, 5mm x 3.2mm, 3.3 V, 7C Series"
				(at 26.035 -24.765 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "24 MHz"
				(at 26.035 -9.525 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "7C-24.000MBB-T"
				(at 26.035 -4.445 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TXC"
				(at 26.035 -6.985 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.035 -19.685 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.035 -22.225 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_24MHz_TXC_7C_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
