(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "R_4x2k2_0201_array"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "R"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "R_4x2k2_0201_array"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "R_4x2k2_0201_array"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://industrial.panasonic.com/cdbs/www-data/pdf/AOC0000/AOC0000C14.pdf"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fixed Network Resistor, 2.2 kohm, Isolated, 4 Resistors, 0502 [1406 Metric], Flat, ± 5%"
				(at 26.67 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EXB-18V222JX"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Panasonic"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "4x2k2_0201"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "0201, SMT, RESISTOR, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "R_4x2k2_0201_array_0_1")
			(symbol "R_4x2k2_0201_array_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "R1.1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "R2.1")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "R3.1")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "R4.1")
					(number "4")
				)
				(pin passive line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "R4.2")
					(number "5")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "R3.2")
					(number "6")
				)
				(pin passive line
					(at 10.16 -2.54 180)
					(length 2.54)
					(name "R2.2")
					(number "7")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "R1.2")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
