(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "C_1u_100V_X7T_0603"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "C"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "C_1u_100V_X7T_0603"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "C_1u_100V_X7T_0603"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://pim.murata.com/en-global/pim/details/?partNum=GRM188D72A105KE01%23"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SMD Multilayer Ceramic Capacitor, 1uF, 100V, 0603, ±10%, X7T"
				(at 15.24 -33.02 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GRM188D72A105KE01J"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Murata"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "1u"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Voltage" "100V"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Dielectric" "X7T"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "C_1u_100V_X7T_0603_0_1")
			(symbol "C_1u_100V_X7T_0603_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.032)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.032)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
