(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L_20n_0.35A_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "L"
				(at 13.97 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "L_20n_0.35A_0402"
				(at 13.97 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L_20n_0.35A_0402"
				(at 13.97 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_automotive_high-frequency_mlg1005s_en.pdf?ref_disty=mouser"
				(at 13.97 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Multilayer Inductor, AEC-Q200, 20 nH, 0.6 ohm, 1.9 GHz, 350 mA, 0402 [1005 Metric], MLG Series"
				(at 13.97 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "20n/0.35A"
				(at 13.97 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TDK"
				(at 13.97 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MLG1005S20NJTD25"
				(at 13.97 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ISat" ""
				(at 13.97 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "IMax" "0.35 A"
				(at 13.97 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Size" "1.0x0.5"
				(at 13.97 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 13.97 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 13.97 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L_20n_0.35A_0402_0_1")
			(symbol "L_20n_0.35A_0402_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.508)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.508)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
