(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "QT6274LW12M-100M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.032 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "QT6274LW12M-100M"
				(at 34.29 -4.572 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "QT6274LW12M-100M"
				(at 34.29 -9.652 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://q-tech.com/wp-content/uploads/QPDS-0115-QT625LW-QT697LW.pdf"
				(at 34.29 -14.732 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "100MHz, Space Qualified Crystal Oscillators,  3.3V, 4 Differential LVDS Pairs"
				(at 34.29 -24.892 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Q-Tech Corporation"
				(at 34.29 -17.272 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "QT6274LW12M-100M"
				(at 34.29 -12.192 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Val" "100 MHz"
				(at 34.29 -7.112 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 34.29 -19.812 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -22.352 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, CLOCK, PCIE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "QT6274LW12M-100M_1_0"
				(pin no_connect line
					(at 2.54 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin output line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "DOUT3+")
					(number "17")
				)
				(pin output line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "DOUT3-")
					(number "18")
				)
				(pin output line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "DOUT4-")
					(number "19")
				)
				(pin output line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "DOUT4+")
					(number "20")
				)
			)
			(symbol "QT6274LW12M-100M_1_1"
				(pin no_connect line
					(at 2.54 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin no_connect line
					(at 2.54 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 2.54 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 2.54 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 2.54 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin no_connect line
					(at 2.54 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin output line
					(at 20.32 0 180)
					(length 2.54)
					(name "DOUT1+")
					(number "11")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "DOUT1-")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "13")
				)
				(pin output line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "DOUT2-")
					(number "14")
				)
				(pin output line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "DOUT2+")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
