(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "R_0R001_WSK2512"
			(pin_numbers
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "R"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "R_0R001_WSK2512"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "R_0R001_WSK2512"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/30108/wsk2512.pdf"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1 mOhms ±1% 1W Chip Resistor 2512 (6432 Metric) Anti-Sulfur, Automotive AEC-Q200, Current Sense, Pulse Withstanding Metal Element"
				(at 20.32 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "WSK25121L000FEA"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Vishay"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "0.001R"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Tolerance" "1%"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RESISTOR, SENSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "R_0R001_WSK2512_0_1")
			(symbol "R_0R001_WSK2512_1_1"
				(pin passive line
					(at 0 -5.08 0)
					(length 0.635)
					(name "I1")
					(number "I1")
				)
				(pin passive line
					(at 7.62 -5.08 180)
					(length 0.635)
					(name "I2")
					(number "I2")
				)
				(pin passive line
					(at 0 0 0)
					(length 0.635)
					(name "V1")
					(number "V1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 0.635)
					(name "V2")
					(number "V2")
				)
			)
			(embedded_fonts no)
		)
)
