(footprint "IND_AMOBEADS_AB4X2X6SM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Noise Suppression 6.00mm W X 8.00mm L X 5.30mm H body")
	(property "Reference" "REF**"
		(at 0 -3.975 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_AMOBEADS_AB4X2X6SM"
		(at 0 3.975 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -5.7 0)
		(size 3.3 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 5.7 0)
		(size 3.3 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
