(footprint "SOIC127P600X160-16N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOIC 16, Pitch 1.27mm, Body 4x10mm, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -6.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC127P600X160-16N"
		(at 0 5.975 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.7 -4.445 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.7 -3.175 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.7 -1.905 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.7 -0.635 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.7 0.635 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.7 1.905 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.7 3.175 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.7 4.445 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.7 4.445 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.7 3.175 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.7 1.905 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.7 0.635 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.7 -0.635 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.7 -1.905 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.7 -3.175 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.7 -4.445 90)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
