(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "RN_VISHAY_VSM46_321189"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RN"
  			(at 3.81 1.778 0)
  		)
  		(property "Value" "${VALUE}"
  			(at 3.81 -1.778 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Bulk Metal® Foil Technology Surface Mount Hermetic Resistor Networks (8 Isolated Resistors), VSM46 Series"
  			(at 0 0 0)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_1_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "529R4"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "1")
  				(number "1")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "16")
  				(number "16")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_2_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "15k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "2")
  				(number "2")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "15")
  				(number "15")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_3_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "1k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "3")
  				(number "3")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "14")
  				(number "14")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_4_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "1k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "4")
  				(number "4")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "13")
  				(number "13")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_5_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "1k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "5")
  				(number "5")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "12")
  				(number "12")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_6_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "1k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "6")
  				(number "6")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "11")
  				(number "11")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_7_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "15k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "7")
  				(number "7")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "10")
  				(number "10")
  			)
  		)
  		(symbol "RN_VISHAY_VSM46_321189_8_0"
  			(text "0.1%"
  				(at 3.81 0 0)
  			)
  			(text "3k"
  				(at 3.81 -2.794 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 1.524)
  				(name "8")
  				(number "8")
  			)
  			(pin passive line
  				(at 7.62 0 180)
  				(length 1.524)
  				(name "9")
  				(number "9")
  			)
  		)
  		(embedded_fonts no)
  	)
)
