(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MP20073DH"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MP20073DH"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MP20073DH"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/2915039.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DDR Termination Regulator, DDR2, DDR3, 1.3V to 6V in, 2A, MSOP-EP-8"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MP20073DH-LF-P"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, DDR, MEMORY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MP20073DH_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DDQ")
					(number "1")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "V_{TT}")
					(number "2")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "V_{TTSEN}")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "V_{DRV}")
					(number "5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "REF")
					(number "6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "V_{TT_EN}")
					(number "7")
				)
				(pin passive line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "V_{TTREF}")
					(number "8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
