(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SI3471A-A01-IMR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 68.58 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SI3471A-A01-IMR"
				(at 68.58 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SI3471A-A01-IMR"
				(at 68.58 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/SL/documents/public/data-sheets/Si3471.pdf"
				(at 68.58 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PoE PSE (Power Sourcing Equipment) integrated circuit, Single port,autonomous, IEEE 802.3bt compliant"
				(at 68.58 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Skyworks Solutions"
				(at 68.58 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI3471A-A01-IMR"
				(at 68.58 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 68.58 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 68.58 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "POE, PMIC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SI3471A-A01-IMR_1_1"
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "LED1")
					(number "1")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "LED2")
					(number "2")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DGND")
					(number "3")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DECPL")
					(number "4")
				)
				(pin output line
					(at 43.18 -8.89 180)
					(length 2.54)
					(name "GATE1")
					(number "5")
				)
				(pin input line
					(at 43.18 -13.97 180)
					(length 2.54)
					(name "SENSE1")
					(number "6")
				)
				(pin input line
					(at 43.18 -3.81 180)
					(length 2.54)
					(name "DRAIN1")
					(number "7")
				)
				(pin input line
					(at 43.18 -20.32 180)
					(length 2.54)
					(name "KSENSE")
					(number "8")
				)
				(pin input line
					(at 43.18 -36.83 180)
					(length 2.54)
					(name "DRAIN2")
					(number "9")
				)
				(pin input line
					(at 43.18 -26.67 180)
					(length 2.54)
					(name "SENSE2")
					(number "10")
				)
				(pin output line
					(at 43.18 -31.75 180)
					(length 2.54)
					(name "GATE2")
					(number "11")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "AGND")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VPWR")
					(number "13")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDA")
					(number "14")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "16")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "17")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "18")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "19")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "20")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "21")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "22")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "23")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "24")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "25")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "26")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "27")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "28")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "DGND")
					(number "29")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD")
					(number "30")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RESETB")
					(number "31")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "32")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MIDB")
					(number "33")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PWRAVL0")
					(number "34")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PWRAVL1")
					(number "35")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PWRAVL2")
					(number "36")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "37")
				)
				(pin no_connect line
					(at 2.54 -34.29 0)
					(length 2.54)
					(hide yes)
					(name "DNC")
					(number "38")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "39")
				)
			)
			(embedded_fonts no)
		)
)
