(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nPM6001-CAXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nPM6001-CAXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-npm:BGA-45_5x9_2.175x3.635mm"
				(at 2.54 -60.96 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_npm6001"
				(at 2.54 -63.5 0)
			)
			(property "Description" "PMIC with Buck/LDO"
				(at 0 -66.04 0)
			)
			(property "ki_keywords" "PMIC Buck Regulator LDO"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA*45*5x9*2.175x3.635mm*"
				(at 0 0 0)
			)
			(symbol "nPM6001-CAXX_0_0"
				(pin bidirectional line
					(at -30.48 33.02 0)
					(length 2.54)
					(name "ENABLE")
					(number "B2")
				)
				(pin bidirectional line
					(at -30.48 27.94 0)
					(length 2.54)
					(name "READY")
					(number "H4")
				)
				(pin bidirectional line
					(at -30.48 22.86 0)
					(length 2.54)
					(name "BUCK_MODE0")
					(number "G2")
				)
				(pin bidirectional line
					(at -30.48 20.32 0)
					(length 2.54)
					(name "BUCK_MODE1")
					(number "F5")
				)
				(pin bidirectional line
					(at -30.48 17.78 0)
					(length 2.54)
					(name "BUCK_MODE2")
					(number "G4")
				)
				(pin power_in line
					(at -30.48 12.7 0)
					(length 2.54)
					(name "VIN_GPIO")
					(number "E1")
				)
				(pin bidirectional line
					(at -30.48 10.16 0)
					(length 2.54)
					(name "GPIO0")
					(number "C2")
				)
				(pin bidirectional line
					(at -30.48 7.62 0)
					(length 2.54)
					(name "GPIO1")
					(number "D3")
				)
				(pin bidirectional line
					(at -30.48 5.08 0)
					(length 2.54)
					(name "GPIO2")
					(number "D2")
				)
				(pin power_in line
					(at -30.48 0 0)
					(length 2.54)
					(name "VDD_TWI")
					(number "C4")
				)
				(pin bidirectional line
					(at -30.48 -2.54 0)
					(length 2.54)
					(name "SDA")
					(number "E2")
				)
				(pin bidirectional line
					(at -30.48 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "E3")
				)
				(pin power_in line
					(at 0 48.26 270)
					(length 2.54)
					(name "VIN")
					(number "G1")
				)
				(pin power_in line
					(at 5.08 48.26 270)
					(length 2.54)
					(name "VIN_BUCK0")
					(number "J5")
				)
				(pin power_in line
					(at 7.62 48.26 270)
					(length 2.54)
					(name "VIN_BUCK1")
					(number "A5")
				)
				(pin power_in line
					(at 10.16 48.26 270)
					(length 2.54)
					(name "VIN_BUCK2")
					(number "A1")
				)
				(pin power_in line
					(at 12.7 48.26 270)
					(length 2.54)
					(name "VIN_BUCK3")
					(number "J1")
				)
				(pin passive line
					(at 30.48 33.02 180)
					(length 2.54)
					(name "SW0")
					(number "J4")
				)
				(pin passive line
					(at 30.48 17.78 180)
					(length 2.54)
					(name "SW1")
					(number "A4")
				)
				(pin power_out line
					(at 30.48 12.7 180)
					(length 2.54)
					(name "VO1")
					(number "B5")
				)
				(pin passive line
					(at 30.48 2.54 180)
					(length 2.54)
					(name "SW2")
					(number "A2")
				)
				(pin power_out line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "VO2")
					(number "B1")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "SW3")
					(number "J2")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "VO3")
					(number "H1")
				)
				(pin power_in line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "VIN_LDO0")
					(number "C1")
				)
				(pin power_out line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "VLDO0")
					(number "D1")
				)
				(pin power_in line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "VIN_LDO1")
					(number "D5")
				)
				(pin power_out line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "VLDO1")
					(number "C5")
				)
			)
			(symbol "nPM6001-CAXX_1_0"
				(pin output line
					(at -30.48 30.48 0)
					(length 2.54)
					(name "~{INT}")
					(number "D4")
				)
				(pin passive line
					(at 0 48.26 270)
					(length 2.54)
					(hide yes)
					(name "VIN_ANA")
					(number "F3")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "AVSS1_2")
					(number "A3")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "B3")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "E5")
				)
				(pin power_in line
					(at 0 -48.26 90)
					(length 2.54)
					(name "VSS")
					(number "F1")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "AVSS_ANA")
					(number "F2")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "F4")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "G3")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "H2")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "AVSS0")
					(number "H3")
				)
				(pin passive line
					(at 0 -48.26 90)
					(length 2.54)
					(hide yes)
					(name "AVSS3")
					(number "J3")
				)
				(pin passive line
					(at 30.48 27.94 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "B4")
				)
				(pin passive line
					(at 30.48 27.94 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "C3")
				)
				(pin passive line
					(at 30.48 27.94 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "E4")
				)
				(pin passive line
					(at 30.48 27.94 180)
					(length 2.54)
					(hide yes)
					(name "VO0_IN")
					(number "G5")
				)
				(pin power_out line
					(at 30.48 27.94 180)
					(length 2.54)
					(name "VO0")
					(number "H5")
				)
			)
			(symbol "nPM6001-CAXX_1_1")
			(embedded_fonts no)
		)
)
