(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "RELS_TYCO_RP78602"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RLS"
  			(at 8.255 1.27 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" ""
  			(at 0 0 0)
  		)
  		(symbol "RELS_TYCO_RP78602_1_0"
  			(pin passive line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "A1")
  				(number "A1")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "C")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at -5.08 -22.86 0)
  				(length 5.08)
  				(name "C")
  				(number "21")
  			)
  			(pin passive line
  				(at 20.32 -5.08 180)
  				(length 5.08)
  				(name "A2")
  				(number "A2")
  			)
  			(pin bidirectional line
  				(at 20.32 -10.16 180)
  				(length 5.08)
  				(name "NC")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at 20.32 -15.24 180)
  				(length 5.08)
  				(name "NO")
  				(number "14")
  			)
  			(pin bidirectional line
  				(at 20.32 -20.32 180)
  				(length 5.08)
  				(name "NC")
  				(number "22")
  			)
  			(pin bidirectional line
  				(at 20.32 -25.4 180)
  				(length 5.08)
  				(name "NO")
  				(number "24")
  			)
  		)
  		(embedded_fonts no)
  	)
)
