(footprint "MK_IM73A135V01XTSA1"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://www.infineon.com/dgdl/Infineon-IM73A135-DataSheet-v01_00-EN.pdf?fileId=8ac78c8c7f2a768a017fadec36b84500")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "MK_IM73A135V01XTSA1"
		(at 0 3.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -0.011 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -0.011 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.76 4.25 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.76 5.45 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.76 6.65 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0.68)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 0.84 -1.5)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "2" smd rect
		(at 0.84 -0.8)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "3" smd rect
		(at -0.86 -1.5)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "4" smd rect
		(at -0.86 -0.8)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "5" smd custom
		(at 0 0.68)
		(size 0.269072 0.269072)
		(drill
			(offset 0.81 0)
		)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -0.81 0)
				(end 0 0)
				(width 0.46)
				(fill no)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_im73a135v01xtsa1.glb"
		(offset
			(xyz -0.011 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
