(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "VEML7700"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 21.082 1.016 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "VEML7700"
				(at 21.082 -4.064 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "VEML7700"
				(at 21.082 -6.604 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.vishay.com/docs/84286/veml7700.pdf"
				(at 21.082 -9.144 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "High Accuracy Ambient Light Sensor with I2C Interface"
				(at 21.082 -11.684 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Vishay"
				(at 21.082 -14.224 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "VEML7700-TT"
				(at 21.082 -1.524 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 21.082 -16.764 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 21.082 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SENSOR, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "VEML7700_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCL")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "2")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
