(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Conn_Molex_SMA_0733910083"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 20.32 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Conn_Molex_SMA_0733910083"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Conn_Molex_SMA_0733910083"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://tools.molex.com/pdm_docs/sd/733910083_sd.pdf"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SMA Connector Jack, Female Socket 50 Ohms Through Hole, Right Angle Solder"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "0733910083"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RECEPTACLE, COAXIAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Conn_Molex_SMA_0733910083_0_0"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "e")
					(number "1")
				)
				(pin passive line
					(at 5.08 -5.08 90)
					(length 2.54)
					(name "SH")
					(number "2")
				)
				(pin passive line
					(at 5.08 -5.08 90)
					(length 2.54)
					(hide yes)
					(name "SH")
					(number "3")
				)
				(pin passive line
					(at 5.08 -5.08 90)
					(length 2.54)
					(hide yes)
					(name "SH")
					(number "4")
				)
				(pin passive line
					(at 5.08 -5.08 90)
					(length 2.54)
					(hide yes)
					(name "SH")
					(number "5")
				)
			)
			(symbol "Conn_Molex_SMA_0733910083_1_1")
			(embedded_fonts no)
		)
)
