(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SW_DPDT_JS202011JCQN_SMD"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "SW"
				(at 20.32 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SW_DPDT_JS202011JCQN_SMD"
				(at 20.32 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "SW_DPDT_JS202011JCQN_SMD"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ckswitches.com/media/1422/js.pdf"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Slide Switch, Subminiature, DPDT, On-On, Surface Mount, JS, 300 mA"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "C&K"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "JS202011JCQN"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SWITCH, SLIDE, DPDT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SW_DPDT_JS202011JCQN_SMD_0_1")
			(symbol "SW_DPDT_JS202011JCQN_SMD_1_1"
				(pin passive line
					(at 10.16 1.27 180)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 10.16 -7.62 180)
					(length 2.54)
					(name "6")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
