(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM4041CIM3-ADJ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM4041CIM3-ADJ"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM4041CIM3-ADJ"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm4041-n.pdf?ts=1705304309065&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FLM4041-N"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Precision micropower shunt voltage reference"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM4041CIM3-ADJ/NOPB"
				(at 33.02 -8.255 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, POWER, SWITCH, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM4041CIM3-ADJ_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin no_connect line
					(at 7.62 0 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "NC")
				)
			)
			(embedded_fonts no)
		)
)
