(footprint "HW-QFN-24_3.5x4.5mm_P0.5mm_NXP_SOT2090-1_SC"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.nxp.com/docs/en/package-information/SOT2090-1(SC).pdf")
	(property "Reference" "REF**"
		(at -2.4 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "HW-QFN-24_3.5x4.5mm_P0.5mm_NXP_SOT2090-1_SC"
		(at -2.73 3.98 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -2.73 5.18 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.73 6.38 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.73 7.58 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "1" smd custom
		(at -1.2 -1.26)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.195 0.885) (xy -0.9505 0.885) (xy -0.9505 0.635) (xy -0.3555 0.635) (xy -0.3555 0.385) (xy -0.9505 0.385)
					(xy -0.9505 0.135) (xy -0.3555 0.135) (xy -0.3555 -0.115) (xy -0.9505 -0.115) (xy -0.9505 -0.365)
					(xy -0.3555 -0.365) (xy -0.3555 -0.613) (xy -0.503 -0.613) (xy -0.503 -0.787) (xy -0.347 -0.943)
					(xy -0.173 -0.943) (xy -0.173 -0.7955) (xy 0.072 -0.7955) (xy 0.072 -1.3905) (xy 0.325 -1.3905)
					(xy 0.325 -0.316) (xy 0.4995 -0.119) (xy 0.4995 0.635) (xy 0.047 0.635)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at -1.625 0)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.9255 0.125) (xy -0.525 0.125) (xy -0.525 -0.125) (xy 0.433 -0.125) (xy 0.6045 -0.297) (xy 0.9255 -0.297)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "5" smd custom
		(at -1.715 0.5)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.43 0.135) (xy -0.435 0.135) (xy -0.435 -0.135) (xy 0.43 -0.135) (xy 0.437 -0.135) (xy 0.444 -0.134)
					(xy 0.451 -0.133) (xy 0.458 -0.132) (xy 0.465 -0.13) (xy 0.472 -0.128) (xy 0.478 -0.126) (xy 0.485 -0.123)
					(xy 0.491 -0.12) (xy 0.498 -0.117) (xy 0.504 -0.113) (xy 0.509 -0.109) (xy 0.515 -0.105) (xy 0.52 -0.1)
					(xy 0.525 -0.095) (xy 0.53 -0.09) (xy 0.535 -0.085) (xy 0.539 -0.079) (xy 0.543 -0.074) (xy 0.547 -0.068)
					(xy 0.55 -0.061) (xy 0.553 -0.055) (xy 0.556 -0.048) (xy 0.558 -0.042) (xy 0.56 -0.035) (xy 0.562 -0.028)
					(xy 0.563 -0.021) (xy 0.564 -0.014) (xy 0.565 -0.007) (xy 0.565 0) (xy 0.565 0.007) (xy 0.564 0.014)
					(xy 0.563 0.021) (xy 0.562 0.028) (xy 0.56 0.035) (xy 0.558 0.042) (xy 0.556 0.048) (xy 0.553 0.055)
					(xy 0.55 0.061) (xy 0.547 0.068) (xy 0.543 0.074) (xy 0.539 0.079) (xy 0.535 0.085) (xy 0.53 0.09)
					(xy 0.525 0.095) (xy 0.52 0.1) (xy 0.515 0.105) (xy 0.509 0.109) (xy 0.504 0.113) (xy 0.498 0.117)
					(xy 0.491 0.12) (xy 0.485 0.123) (xy 0.478 0.126) (xy 0.472 0.128) (xy 0.465 0.13) (xy 0.458 0.132)
					(xy 0.451 0.133) (xy 0.444 0.134) (xy 0.437 0.135) (xy 0.43 0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "6" smd custom
		(at -1.715 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.43 0.135) (xy -0.435 0.135) (xy -0.435 -0.135) (xy 0.43 -0.135) (xy 0.437 -0.135) (xy 0.444 -0.134)
					(xy 0.451 -0.133) (xy 0.458 -0.132) (xy 0.465 -0.13) (xy 0.472 -0.128) (xy 0.478 -0.126) (xy 0.485 -0.123)
					(xy 0.491 -0.12) (xy 0.498 -0.117) (xy 0.504 -0.113) (xy 0.509 -0.109) (xy 0.515 -0.105) (xy 0.52 -0.1)
					(xy 0.525 -0.095) (xy 0.53 -0.09) (xy 0.535 -0.085) (xy 0.539 -0.079) (xy 0.543 -0.074) (xy 0.547 -0.068)
					(xy 0.55 -0.061) (xy 0.553 -0.055) (xy 0.556 -0.048) (xy 0.558 -0.042) (xy 0.56 -0.035) (xy 0.562 -0.028)
					(xy 0.563 -0.021) (xy 0.564 -0.014) (xy 0.565 -0.007) (xy 0.565 0) (xy 0.565 0.007) (xy 0.564 0.014)
					(xy 0.563 0.021) (xy 0.562 0.028) (xy 0.56 0.035) (xy 0.558 0.042) (xy 0.556 0.048) (xy 0.553 0.055)
					(xy 0.55 0.061) (xy 0.547 0.067) (xy 0.543 0.074) (xy 0.539 0.079) (xy 0.535 0.085) (xy 0.53 0.09)
					(xy 0.525 0.095) (xy 0.52 0.1) (xy 0.515 0.105) (xy 0.509 0.109) (xy 0.504 0.113) (xy 0.498 0.117)
					(xy 0.491 0.12) (xy 0.485 0.123) (xy 0.478 0.126) (xy 0.472 0.128) (xy 0.465 0.13) (xy 0.458 0.132)
					(xy 0.451 0.133) (xy 0.444 0.134) (xy 0.437 0.135) (xy 0.43 0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "7" smd custom
		(at -1.715 1.5)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.43221 0.135) (xy -0.436 0.135) (xy -0.436 -0.135) (xy 0.405 -0.135) (xy 0.412 -0.135) (xy 0.419 -0.134)
					(xy 0.426 -0.133) (xy 0.433 -0.132) (xy 0.439 -0.13) (xy 0.446 -0.128) (xy 0.453 -0.126) (xy 0.459 -0.123)
					(xy 0.466 -0.12) (xy 0.472 -0.117) (xy 0.478 -0.113) (xy 0.484 -0.109) (xy 0.489 -0.105) (xy 0.495 -0.1)
					(xy 0.5 -0.095) (xy 0.505 -0.09) (xy 0.509 -0.085) (xy 0.514 -0.079) (xy 0.518 -0.074) (xy 0.521 -0.067)
					(xy 0.525 -0.061) (xy 0.528 -0.055) (xy 0.531 -0.048) (xy 0.533 -0.042) (xy 0.535 -0.035) (xy 0.537 -0.028)
					(xy 0.538 -0.021) (xy 0.539 -0.014) (xy 0.539 -0.007) (xy 0.54 0) (xy 0.54 0.027) (xy 0.432 0.135)
					(xy 0.43221 0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "8" smd custom
		(at -1 2.225)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.703 -0.352) (xy -0.703 -0.178) (xy -0.547 -0.022) (xy -0.373 -0.022) (xy -0.373 -0.17) (xy -0.135 -0.17)
					(xy -0.135 0.425) (xy 0.135 0.425) (xy 0.135 -0.415) (xy 0.135 -0.422) (xy 0.134 -0.429) (xy 0.133 -0.436)
					(xy 0.132 -0.443) (xy 0.13 -0.45) (xy 0.128 -0.457) (xy 0.126 -0.463) (xy 0.123 -0.47) (xy 0.12 -0.476)
					(xy 0.117 -0.482) (xy 0.113 -0.489) (xy 0.109 -0.494) (xy 0.105 -0.5) (xy 0.1 -0.505) (xy 0.095 -0.51)
					(xy 0.09 -0.515) (xy 0.085 -0.52) (xy 0.079 -0.524) (xy 0.074 -0.528) (xy 0.068 -0.532) (xy 0.061 -0.535)
					(xy 0.055 -0.538) (xy 0.048 -0.541) (xy 0.042 -0.543) (xy 0.035 -0.545) (xy 0.028 -0.547) (xy 0.021 -0.548)
					(xy 0.014 -0.549) (xy 0.007 -0.55) (xy 0 -0.55) (xy -0.027 -0.55) (xy -0.135 -0.442) (xy -0.135 -0.352)
					(xy -0.703 -0.352)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "9" smd custom
		(at -0.5 2.225)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.135 -0.44) (xy -0.135 0.425) (xy 0.135 0.425) (xy 0.135 -0.44) (xy 0.135 -0.447) (xy 0.134 -0.454)
					(xy 0.133 -0.461) (xy 0.132 -0.468) (xy 0.13 -0.475) (xy 0.128 -0.482) (xy 0.126 -0.488) (xy 0.123 -0.495)
					(xy 0.12 -0.501) (xy 0.117 -0.508) (xy 0.113 -0.514) (xy 0.109 -0.519) (xy 0.105 -0.525) (xy 0.1 -0.53)
					(xy 0.095 -0.535) (xy 0.09 -0.54) (xy 0.085 -0.545) (xy 0.079 -0.549) (xy 0.074 -0.553) (xy 0.068 -0.557)
					(xy 0.061 -0.56) (xy 0.055 -0.563) (xy 0.048 -0.566) (xy 0.042 -0.568) (xy 0.035 -0.57) (xy 0.028 -0.572)
					(xy 0.021 -0.573) (xy 0.014 -0.574) (xy 0.007 -0.575) (xy 0 -0.575) (xy -0.007 -0.575) (xy -0.014 -0.574)
					(xy -0.021 -0.573) (xy -0.028 -0.572) (xy -0.035 -0.57) (xy -0.042 -0.568) (xy -0.048 -0.566) (xy -0.055 -0.563)
					(xy -0.061 -0.56) (xy -0.068 -0.557) (xy -0.074 -0.553) (xy -0.079 -0.549) (xy -0.085 -0.545) (xy -0.09 -0.54)
					(xy -0.095 -0.535) (xy -0.1 -0.53) (xy -0.105 -0.525) (xy -0.109 -0.519) (xy -0.113 -0.514) (xy -0.117 -0.508)
					(xy -0.12 -0.501) (xy -0.123 -0.495) (xy -0.126 -0.488) (xy -0.128 -0.482) (xy -0.13 -0.475) (xy -0.132 -0.468)
					(xy -0.133 -0.461) (xy -0.134 -0.454) (xy -0.135 -0.447) (xy -0.135 -0.44)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "10" smd custom
		(at 0 2.225)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.211 -1.051) (xy -0.6 -1.4395) (xy -0.6 -1.7745) (xy 0.6 -1.7745) (xy 0.6 -1.4395) (xy 0.211 -1.051)
					(xy 0.211 -0.679) (xy 0.125 -0.593) (xy 0.125 0.425) (xy -0.125 0.425) (xy -0.125 -0.593) (xy -0.211 -0.679)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "11" smd custom
		(at 0.5 2.225)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.135 0.425) (xy -0.135 0.425) (xy -0.135 -0.44) (xy -0.135 -0.447) (xy -0.134 -0.454) (xy -0.133 -0.461)
					(xy -0.132 -0.468) (xy -0.13 -0.475) (xy -0.128 -0.482) (xy -0.126 -0.488) (xy -0.123 -0.495) (xy -0.12 -0.501)
					(xy -0.117 -0.508) (xy -0.113 -0.514) (xy -0.109 -0.519) (xy -0.105 -0.525) (xy -0.1 -0.53) (xy -0.095 -0.535)
					(xy -0.09 -0.54) (xy -0.085 -0.545) (xy -0.079 -0.549) (xy -0.074 -0.553) (xy -0.068 -0.557) (xy -0.061 -0.56)
					(xy -0.055 -0.563) (xy -0.048 -0.566) (xy -0.042 -0.568) (xy -0.035 -0.57) (xy -0.028 -0.572) (xy -0.021 -0.573)
					(xy -0.014 -0.574) (xy -0.007 -0.575) (xy 0 -0.575) (xy 0.007 -0.575) (xy 0.014 -0.574) (xy 0.021 -0.573)
					(xy 0.028 -0.572) (xy 0.035 -0.57) (xy 0.042 -0.568) (xy 0.048 -0.566) (xy 0.055 -0.563) (xy 0.061 -0.56)
					(xy 0.068 -0.557) (xy 0.074 -0.553) (xy 0.079 -0.549) (xy 0.085 -0.545) (xy 0.09 -0.54) (xy 0.095 -0.535)
					(xy 0.1 -0.53) (xy 0.105 -0.525) (xy 0.109 -0.519) (xy 0.113 -0.514) (xy 0.117 -0.508) (xy 0.12 -0.501)
					(xy 0.123 -0.495) (xy 0.126 -0.488) (xy 0.128 -0.482) (xy 0.13 -0.475) (xy 0.132 -0.468) (xy 0.133 -0.461)
					(xy 0.134 -0.454) (xy 0.135 -0.447) (xy 0.135 -0.44) (xy 0.135 0.425)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "12" smd custom
		(at 1 2.225)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.135 -0.415) (xy -0.135 0.425) (xy 0.135 0.425) (xy 0.135 -0.17) (xy 0.373 -0.17) (xy 0.373 -0.022)
					(xy 0.547 -0.022) (xy 0.703 -0.178) (xy 0.703 -0.352) (xy 0.135 -0.352) (xy 0.135 -0.442) (xy 0.027 -0.55)
					(xy 0 -0.55) (xy -0.007 -0.55) (xy -0.014 -0.549) (xy -0.021 -0.548) (xy -0.028 -0.547) (xy -0.035 -0.545)
					(xy -0.042 -0.543) (xy -0.048 -0.541) (xy -0.055 -0.538) (xy -0.061 -0.535) (xy -0.068 -0.532)
					(xy -0.074 -0.528) (xy -0.079 -0.524) (xy -0.085 -0.52) (xy -0.09 -0.515) (xy -0.095 -0.51) (xy -0.1 -0.505)
					(xy -0.105 -0.5) (xy -0.109 -0.494) (xy -0.113 -0.489) (xy -0.117 -0.482) (xy -0.12 -0.476) (xy -0.123 -0.47)
					(xy -0.126 -0.463) (xy -0.128 -0.457) (xy -0.13 -0.45) (xy -0.132 -0.443) (xy -0.133 -0.436) (xy -0.134 -0.429)
					(xy -0.135 -0.422) (xy -0.135 -0.415)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "13" smd custom
		(at 1.715 1.5)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.43221 0.135) (xy -0.54 0.027) (xy -0.54 0) (xy -0.539 -0.007) (xy -0.539 -0.014) (xy -0.538 -0.021)
					(xy -0.537 -0.028) (xy -0.535 -0.035) (xy -0.533 -0.042) (xy -0.531 -0.048) (xy -0.528 -0.055)
					(xy -0.525 -0.061) (xy -0.521 -0.067) (xy -0.518 -0.074) (xy -0.514 -0.079) (xy -0.509 -0.085)
					(xy -0.505 -0.09) (xy -0.5 -0.095) (xy -0.495 -0.1) (xy -0.489 -0.105) (xy -0.484 -0.109) (xy -0.478 -0.113)
					(xy -0.472 -0.117) (xy -0.466 -0.12) (xy -0.459 -0.123) (xy -0.453 -0.126) (xy -0.446 -0.128) (xy -0.439 -0.13)
					(xy -0.433 -0.132) (xy -0.426 -0.133) (xy -0.419 -0.134) (xy -0.412 -0.135) (xy -0.405 -0.135)
					(xy 0.436 -0.135) (xy 0.436 0.135) (xy -0.432 0.135) (xy -0.43221 0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "14" smd custom
		(at 1.715 1)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.43 -0.135) (xy 0.435 -0.135) (xy 0.435 0.135) (xy -0.43 0.135) (xy -0.437 0.135) (xy -0.444 0.134)
					(xy -0.451 0.133) (xy -0.458 0.132) (xy -0.465 0.13) (xy -0.472 0.128) (xy -0.478 0.126) (xy -0.485 0.123)
					(xy -0.491 0.12) (xy -0.497 0.117) (xy -0.504 0.113) (xy -0.509 0.109) (xy -0.515 0.105) (xy -0.52 0.1)
					(xy -0.525 0.095) (xy -0.53 0.09) (xy -0.535 0.085) (xy -0.539 0.079) (xy -0.543 0.074) (xy -0.547 0.067)
					(xy -0.55 0.061) (xy -0.553 0.055) (xy -0.556 0.048) (xy -0.558 0.042) (xy -0.56 0.035) (xy -0.562 0.028)
					(xy -0.563 0.021) (xy -0.564 0.014) (xy -0.565 0.007) (xy -0.565 0) (xy -0.565 -0.007) (xy -0.564 -0.014)
					(xy -0.563 -0.021) (xy -0.562 -0.028) (xy -0.56 -0.035) (xy -0.558 -0.042) (xy -0.556 -0.048) (xy -0.553 -0.055)
					(xy -0.55 -0.061) (xy -0.547 -0.068) (xy -0.543 -0.074) (xy -0.539 -0.079) (xy -0.535 -0.085) (xy -0.53 -0.09)
					(xy -0.525 -0.095) (xy -0.52 -0.1) (xy -0.515 -0.105) (xy -0.509 -0.109) (xy -0.504 -0.113) (xy -0.497 -0.117)
					(xy -0.491 -0.12) (xy -0.485 -0.123) (xy -0.478 -0.126) (xy -0.472 -0.128) (xy -0.465 -0.13) (xy -0.458 -0.132)
					(xy -0.451 -0.133) (xy -0.444 -0.134) (xy -0.437 -0.135) (xy -0.43 -0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "15" smd custom
		(at 1.715 0.5)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.43 -0.135) (xy 0.435 -0.135) (xy 0.435 0.135) (xy -0.43 0.135) (xy -0.437 0.135) (xy -0.444 0.134)
					(xy -0.451 0.133) (xy -0.458 0.132) (xy -0.465 0.13) (xy -0.472 0.128) (xy -0.478 0.126) (xy -0.485 0.123)
					(xy -0.491 0.12) (xy -0.498 0.117) (xy -0.504 0.113) (xy -0.509 0.109) (xy -0.515 0.105) (xy -0.52 0.1)
					(xy -0.525 0.095) (xy -0.53 0.09) (xy -0.535 0.085) (xy -0.539 0.079) (xy -0.543 0.074) (xy -0.547 0.068)
					(xy -0.55 0.061) (xy -0.553 0.055) (xy -0.556 0.048) (xy -0.558 0.042) (xy -0.56 0.035) (xy -0.562 0.028)
					(xy -0.563 0.021) (xy -0.564 0.014) (xy -0.565 0.007) (xy -0.565 0) (xy -0.565 -0.007) (xy -0.564 -0.014)
					(xy -0.563 -0.021) (xy -0.562 -0.028) (xy -0.56 -0.035) (xy -0.558 -0.042) (xy -0.556 -0.048) (xy -0.553 -0.055)
					(xy -0.55 -0.061) (xy -0.547 -0.068) (xy -0.543 -0.074) (xy -0.539 -0.079) (xy -0.535 -0.085) (xy -0.53 -0.09)
					(xy -0.525 -0.095) (xy -0.52 -0.1) (xy -0.515 -0.105) (xy -0.509 -0.109) (xy -0.504 -0.113) (xy -0.497 -0.117)
					(xy -0.491 -0.12) (xy -0.485 -0.123) (xy -0.478 -0.126) (xy -0.472 -0.128) (xy -0.465 -0.13) (xy -0.458 -0.132)
					(xy -0.451 -0.133) (xy -0.444 -0.134) (xy -0.437 -0.135) (xy -0.43 -0.135)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "16" smd custom
		(at 1.625 0)
		(size 1 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.525 0.125) (xy -0.9255 0.125) (xy -0.9255 -0.297) (xy -0.6045 -0.297) (xy -0.433 -0.125)
					(xy 0.525 -0.125)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "17" smd custom
		(at 1.2 -1.26)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.047 0.635) (xy -0.4995 0.635) (xy -0.4995 -0.119) (xy -0.325 -0.316) (xy -0.325 -1.3905)
					(xy -0.072 -1.3905) (xy -0.072 -0.7955) (xy 0.173 -0.7955) (xy 0.173 -0.943) (xy 0.347 -0.943)
					(xy 0.503 -0.787) (xy 0.503 -0.613) (xy 0.3555 -0.613) (xy 0.3555 -0.365) (xy 0.9505 -0.365) (xy 0.9505 -0.115)
					(xy 0.3555 -0.115) (xy 0.3555 0.135) (xy 0.9505 0.135) (xy 0.9505 0.385) (xy 0.3555 0.385) (xy 0.3555 0.635)
					(xy 0.9505 0.635) (xy 0.9505 0.885) (xy 0.195 0.885)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "21" smd custom
		(at 0 -0.95)
		(size 0.5 2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.625 -1.7005) (xy -0.625 -0.798) (xy -0.38 -0.553) (xy -0.38 1.075) (xy 0.38 1.075) (xy 0.38 -0.553)
					(xy 0.625 -0.798) (xy 0.625 -1.7005) (xy 0.375 -1.7005) (xy 0.375 -1.1055) (xy 0.125 -1.1055) (xy 0.125 -1.7005)
					(xy -0.125 -1.7005) (xy -0.125 -1.1055) (xy -0.375 -1.1055) (xy -0.375 -1.7005)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_mpf5302amda0es.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
