(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NCP51400MNTXG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NCP51400MNTXG"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NCP51400MNTXG"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/NCP51400_D-1812533.pdf"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fixed LDO Voltage Regulator, 2.375V to 5.5V, 1.2 V Drop, 750 mV/3A out, DFN-10 Pins"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NCP51400MNTXG"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DFN10_3X3_ONS DFN10_3X3_ONS-M DFN10_3X3_ONS-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NCP51400MNTXG_1_1"
				(pin unspecified line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VRI")
					(number "1")
				)
				(pin unspecified line
					(at 0 -8.89 0)
					(length 2.54)
					(name "PVCC")
					(number "2")
				)
				(pin unspecified line
					(at 24.13 -3.81 180)
					(length 2.54)
					(name "VTT")
					(number "3")
				)
				(pin power_in line
					(at 10.16 -22.86 90)
					(length 2.54)
					(name "PGND")
					(number "4")
				)
				(pin unspecified line
					(at 24.13 -6.35 180)
					(length 2.54)
					(name "VTTS")
					(number "5")
				)
				(pin unspecified line
					(at 24.13 -17.78 180)
					(length 2.54)
					(name "VRO")
					(number "6")
				)
				(pin unspecified line
					(at 0 -6.35 0)
					(length 2.54)
					(name "EN")
					(number "7")
				)
				(pin power_in line
					(at 12.7 -22.86 90)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 2.54)
					(name "PGOOD")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
				(pin unspecified line
					(at 15.24 -22.86 90)
					(length 2.54)
					(name "EPAD")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
