(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SW_SDA04H1SBD"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "SW"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SW_SDA04H1SBD"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SW_SDA04H1SBD"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ckswitches.com/media/1327/sda.pdf"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dip Switch SPST 4 Position Surface Mount Slide (Standard) Actuator 25mA 24VDC"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SDA04H1SBD"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "C&K"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SWITCH, MECHANICAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SW?DIP?x2*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SW_SDA04H1SBD_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "A1")
					(number "A1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A2")
					(number "A2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A3")
					(number "A3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A4")
					(number "A4")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "B1")
					(number "B1")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "B2")
					(number "B2")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "B3")
					(number "B3")
				)
				(pin passive line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "B4")
					(number "B4")
				)
			)
			(embedded_fonts no)
		)
)
