(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SW_SKRHADE010_SMD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "SW"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SW_SKRHADE010_SMD"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SW_SKRHADE010_SMD"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.rs-online.com/a1d6/0900766b8152c2fa.pdf"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pushbutton Switches 4-direct, center push w/ boss 500K cycles"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SKRHADE010"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Alps Alpine"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SWITCH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SW_SKRHADE010_SMD_1_1"
				(pin passive line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 16.51 0 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "C")
					(number "3")
				)
				(pin passive line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "B")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 16.51 -10.16 180)
					(length 2.54)
					(name "D")
					(number "6")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
