(footprint "PB_C&K_8121SD9AGE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Right Angled SPDT Snap-acting Momentary Pushbuttom Switch, Unthreaded Bushing, Contact Rating 1A 120VAC or 28VDC, 8020 Series")
	(property "Reference" "REF**"
		(at -12.3282 -7.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_C&K_8121SD9AGE"
		(at -12.3282 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at 0 4.7 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0 -4.7 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -12.7 -2.54)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -12.7 2.54)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -12.6968 4.87353) (xy -12.6968 3.99031) (xy -12.69649 3.99) (xy -11.24649 3.99) (xy -11.24649 1.09) (xy -12.69649 1.09) (xy -12.69649 -1.09) (xy -11.24649 -1.09) (xy -11.24649 -3.99) (xy -12.69649 -3.99) (xy -12.69649 -4.87367) (xy -3.67038 -4.87367) (xy -3.66725 -4.87054) (xy -3.66725 4.87666)
			)
		)
	)
	(embedded_fonts no)
)
