(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "PB_CTS_228ADS2ARGFCMBA"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "PB"
  			(at 7.62 5.08 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Push-Button Switch SPDT + 2x led"
  			(at 0 0 0)
  		)
  		(symbol "PB_CTS_228ADS2ARGFCMBA_1_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at 0 -2.54 0)
  				(length 4.445)
  				(name "C")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "NO")
  				(number "4")
  			)
  		)
  		(symbol "PB_CTS_228ADS2ARGFCMBA_2_0"
  			(pin bidirectional line
  				(at -1.27 0 0)
  				(length 5.08)
  				(name "L1")
  				(number "L1")
  			)
  			(pin bidirectional line
  				(at 16.51 0 180)
  				(length 5.08)
  				(name "L2")
  				(number "L2")
  			)
  		)
  		(embedded_fonts no)
  	)
)
