(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_ALPS_EC11B15242AE"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 6.35 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 6.985 -11.43 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Encoder, 30-Detent, 15-Pulse, Horizontal With Push-on Switch"
  			(at 0 0 0)
  		)
  		(symbol "SW_ALPS_EC11B15242AE_1_0"
  			(pin passive line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "A")
  				(number "1")
  			)
  			(pin passive line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "C")
  				(number "3")
  			)
  			(pin passive line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "B")
  				(number "2")
  			)
  			(pin passive line
  				(at 17.78 -2.54 180)
  				(length 5.08)
  				(name "D")
  				(number "4")
  			)
  			(pin passive line
  				(at 17.78 -7.62 180)
  				(length 5.08)
  				(name "E")
  				(number "5")
  			)
  		)
  		(symbol "SW_ALPS_EC11B15242AE_2_0")
  		(symbol "SW_ALPS_EC11B15242AE_3_0")
  		(embedded_fonts no)
  	)
)
