(footprint "SW_APEM_IKN0403000"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Pitch 2.54mm,  Body 11.1x7.30mm, 4 Ways SPST Surface-Mount DIP Switch, APEM INK Series")
	(property "Reference" "REF**"
		(at 0 -6.445 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_IKN0403000"
		(at 0 6.445 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "3"
		(at -3.298 1 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -3.298 3.5 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -3.298 -3.9 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -3.298 -1.5 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 2.302 -4.5 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 2.302 -4.5 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -3.298 -3.9 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -3.298 -1.5 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -3.298 3.5 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -3.298 1 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.695 -3.81)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.695 -1.27)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.695 1.27)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.695 3.81)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 4.695 3.81)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 4.695 1.27)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.695 -1.27)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.695 -3.81)
		(size 1.77 1.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
