(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_APEM_MU-AS90R"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 7.62 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Multidirectional Switch 5 Way (4-directional and center push)"
  			(at 0 0 0)
  		)
  		(symbol "SW_APEM_MU-AS90R_1_0"
  			(text "A"
  				(at 1.27 -1.27 0)
  			)
  			(text "B"
  				(at 1.27 -6.35 0)
  			)
  			(text "C"
  				(at 1.27 -11.43 0)
  			)
  			(text "COM"
  				(at 12.7 -13.716 0)
  			)
  			(text "(Center)F"
  				(at 13.97 -1.27 0)
  			)
  			(text "E"
  				(at 13.97 -6.35 0)
  			)
  			(text "D"
  				(at 13.97 -11.43 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "A")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "E")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "C")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 20.32 -2.54 180)
  				(length 5.08)
  				(name "D")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at 20.32 -7.62 180)
  				(length 5.08)
  				(name "COM")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at 20.32 -12.7 180)
  				(length 5.08)
  				(name "B")
  				(number "6")
  			)
  		)
  		(embedded_fonts no)
  	)
)
