(footprint "SW_CTS_204-121ST"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 7.26 x 9.78mm SPDT DIP Switch, 204 Series")
	(property "Reference" "REF**"
		(at -0.29 -4.605 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_CTS_204-121ST"
		(at -0.29 4.605 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -5.86 -2.3765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -5.859 -2.3815 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.3 -1.26995 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.3 1.27004 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 4.3 1.27004 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 4.3 -1.26995 270)
		(size 1.13 2.44)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
