(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_E-SWITCH_1004P3T2B4M7QE"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 5.08 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Right Angle 4PDT Toggle Switch ON-OFF-ON, Contact Rating 20V 0.4VAC, Contact Gold, 100 Series"
  			(at 0 0 0)
  		)
  		(symbol "SW_E-SWITCH_1004P3T2B4M7QE_1_0"
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "C")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "C")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at -5.08 -25.4 0)
  				(length 5.08)
  				(name "C")
  				(number "8")
  			)
  			(pin bidirectional line
  				(at -5.08 -35.56 0)
  				(length 5.08)
  				(name "C")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 5.08)
  				(name "NC")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at 15.24 -7.62 180)
  				(length 5.08)
  				(name "NO")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 15.24 -12.7 180)
  				(length 5.08)
  				(name "NC")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at 15.24 -17.78 180)
  				(length 5.08)
  				(name "NO")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at 15.24 -22.86 180)
  				(length 5.08)
  				(name "NC")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at 15.24 -27.94 180)
  				(length 5.08)
  				(name "NO")
  				(number "9")
  			)
  			(pin bidirectional line
  				(at 15.24 -33.02 180)
  				(length 5.08)
  				(name "NC")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at 15.24 -38.1 180)
  				(length 5.08)
  				(name "NO")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at 15.24 -43.18 180)
  				(length 5.08)
  				(name "NO")
  				(number "MECH1")
  			)
  			(pin bidirectional line
  				(at 15.24 -45.72 180)
  				(length 5.08)
  				(name "NO")
  				(number "MECH2")
  			)
  		)
  		(embedded_fonts no)
  	)
)
