(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_NKK_B12JJVC"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 5.08 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "SPDT ON NONE ON Red Illuminated Switch"
  			(at 0 0 0)
  		)
  		(symbol "SW_NKK_B12JJVC_1_0"
  			(text "RED"
  				(at 5.08 -13.208 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "2")
  				(number "2")
  			)
  			(pin passive line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "5")
  				(number "5")
  			)
  			(pin passive line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "7")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 5.08)
  				(name "3")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 15.24 -7.62 180)
  				(length 5.08)
  				(name "1")
  				(number "1")
  			)
  			(pin passive line
  				(at 15.24 -10.16 180)
  				(length 5.08)
  				(name "6")
  				(number "6")
  			)
  			(pin passive line
  				(at 15.24 -12.7 180)
  				(length 5.08)
  				(name "8")
  				(number "8")
  			)
  		)
  		(embedded_fonts no)
  	)
)
